	Last updated
	equipment
	fault
	Action required
	

	15/06/2026
	Litter bins
	Requires emptying. Risk 6
	Regular emptying assigned
to
	monitor

	15/06/2026
	Bench in play area
	Requires painting. Risk 2
	Volunteer assigned to paint
	COMPLETE

	15/06/2026
	Cableway flooring
	Floor needs replacing/repair.  Risk 7
	Awaiting other floor areas to be repaired before getting quotes for this area
	monitor

	15/06/2026
	Cableway chain links
	To be inspected for wear and tear. Risk 4
	Assign a specialist company
	Kompany contacted 10/06

	15/06/2026
	Floor at goalposts
	This is worn and needs reseeding. Risk 8
	Goal post to be moved for the winter months
	monitor

	15/06/2026
	Goalposts
	EN 748 /EN 16579 Structural tests are required. Risk not recorded.
	
	

	15/06/2026
	Goalposts
	Algae and dirt discovered on posts. Posts require painting.  Risk 2
	Posts to be cleaned
	monitor

	15/06/2026
	MAGU
	Sign required to show who and how it should be used. Risk 5
	Sign already in place to be lowered
	Sign lowering to be assigned

	15/06/2026
	MAGU
	Bolts were found to be loose on the fencing. Risk 10
	Bolts to be tightened
	COMPLETE

	23/06/2026
	MAGU
	The goal netting eye bolts needs to be tightened. Risk 5
	Repair required if netting becomes loose
	COMPLETE

	15/06/2026
	Basketball court
	Sign required to show who and how it should be used. Risk 5
	Sign already in the area needs to be lowered
	Sign lowering to be assigned

	15/06/2026
	Basketball court
	The surface is cracking. Risk 6
	Risk is low
	monitor

	15/06/2026
	Swing Group
	This should be checked to manufacturer’s instructions. Risk 6
	Assign to specialist company
	Kompany contacted 10/06

	15/06/2026
	Space net
	There is several trip points around the anchor base structure. Risk 6
	Assign to a specialist company
	Kompany contacted 10/06

	15/06/2026
	Space net
	The tension on the space net should be checked as per manufactures instruction. Risk 6
	Assign to a specialist company
	Kompany contacted 10/06

	15/06/2026
	Swing contact
	This should be inspected as per the manufacture’s instructions. Risk 5
	Assign to a specialist company
	Kompany contacted 10/06

	22/06/2026
	Mixed 2 bay junior swing
	Bolts are too long. Risk 8
	Bolts to be adjusted so the bolt is nearer the end. KM
	COMPLETED

	15/06/2026
	Carousel
	There is a lip on carousel which has dropped. Risk 8
	Assign to a specialist company
	Kompany contacted 10/06

	15/06/2026
	Play panels
	The hedge is intruding. Risk 6
	Requires to be cut back
	Will be cut back when season permits

	15/06/2026
	Play panels
	Graffiti to be removed. Risk 1
	Graffiti is removed
	COMPLETE

	15/06/2026
	Rocker
	Two missing caps from the underside to be replaced. Risk 3
	Caps have been replaced
	COMPLETE

	15/06/2026
	Toddler Multiplay
	The climbing rope is loose at the top. Risk 8
	Could find no fault
	COMPLETE

	23/06/2026
	Toddler Multiplay
	Play dials are stiff and difficult to move. Risk 2
	To be loosened KM to investigate further
	COMPLETE

	15/06/2026
	Gate to play area
	Gate is not closing as required. Risk 6
	No fault found
	COMPLETE

	
	
	
	
	



